(module USB_microB (layer F.Cu) (tedit 5778AF29)
  (descr "USB microB hirose ZX62R-B-5P")
  (tags "USB micorB hirose")
  (fp_text reference J** (at 0 -0.6985) (layer F.SilkS)
    (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
  )
  (fp_text value USB_microB (at 0 0.22606) (layer F.SilkS) hide
    (effects (font (size 0.6 0.6) (thickness 0.15)))
  )
  (fp_text user "PCB edge" (at -0.05 1.45) (layer F.SilkS) hide
    (effects (font (size 0.5 0.5) (thickness 0.125)))
  )
  (fp_line (start 3.75 2.15) (end 4.25 2.75) (layer Dwgs.User) (width 0.2))
  (fp_line (start -3.75 2.15) (end -4.25 2.675) (layer Dwgs.User) (width 0.2))
  (fp_line (start -3 1.45) (end 3 1.45) (layer Dwgs.User) (width 0.2))
  (fp_line (start -3.75 2.15) (end -3.75 1.35) (layer Dwgs.User) (width 0.2))
  (fp_line (start -3.75 2.15) (end 3.75 2.15) (layer Dwgs.User) (width 0.2))
  (fp_line (start 3.75 2.15) (end 3.75 1.35) (layer Dwgs.User) (width 0.2))
  (pad 6 smd rect (at 0.85 0) (size 1.2 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 1.29794 -2.67462 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
    (clearance 0.1))
  (pad 6 smd rect (at -3.0988 -2.3495) (size 2.1 2) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 3.0988 -2.3495) (size 2.1 2) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -4.09956 0) (size 1.6 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 4.09956 0) (size 1.6 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.65024 -2.67462 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
    (clearance 0.1))
  (pad 3 smd rect (at 0 -2.67462 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
    (clearance 0.1))
  (pad 4 smd rect (at -0.65024 -2.67462 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
    (clearance 0.1))
  (pad 5 smd rect (at -1.30048 -2.67462 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
    (clearance 0.1))
  (pad 6 smd rect (at -0.85 0) (size 1.2 1.9) (layers F.Cu F.Paste F.Mask))
)
